Afzaal, M, Yates, HM, Walter, A, Nicolay, S, Ballif, C, "1 cm2 CH3NH3PbI3 mesoporous solar cells with 17.8% steady-state efficiency by tailoring front FTO electrodes", Journal of Materials Chemistry C, 2017